

**SNMP Configuration for TIP OLTs**

1. **Vendor: Netlink** and **Syrotech**

**Device Information**



**Before Configuration:** For SNMP Disabled cases, the IPv4 SNMP will be in **DENY** state.



**For Configuration:** **Select following details and then ADD**

Filter Action - Permit

Internet Version – IPv4


Protocol – SNMP

Source IP – 172.30.6.0

IP Mask – 255.255.255.0

Similarly, ADD for Source IP – 172.30.22.0 and IP Mask – 255.255.255.128

**After Configuration:** For the SNMP Enabled cases, the SNMP will be in **Permit** state for the BBNMS IP Pools.



1. **Vendor: Electroline** and **Richerlink**

**Device Information**



**Before Configuration:** For SNMP Disabled cases, SNMP Group Management 🡪 **GROUP PROFILE** will be having no details regarding **GROUP NAME**

**For Configuration:**

SNMP Group Management 🡪 **GROUP NAME = public 🡪 Access = ro 🡪 ADD**

**After Configuration:**

For SNMP Enabled cases, SNMP Group Management 🡪 **GROUP PROFILE** will be having details regarding **GROUP NAME** as **public** with access as **ro (read only)**

